Computer Installation at Eceau Ltd
Updated:  Tuesday, 9 August 2016		Contact: Barnaby Foster			

Business Address:	
Greenhills Estate
Tilford Road
Tilford
Farnham
Surrey 
GU10 2DZ

Telephone:	01252 758933
Web: 	http://eceaultd.co.uk 
email:	barnabyf@eceaultd.co.uk 


Router No.1
Model Name: Vigor2860Vac 
Firmware Version: 3.8.2.3_BT 
Build Date/Time: Apr 22 2016 19:28:07 
Access: http://192.168.1.1  
Userid: admin		Password: darwin31415 
Broadband Service from BT
Username: D458423@hg70.btclick.com		Password: welcome1
Phone Number: 01252 793804
Fixed IP: 81.136.214.64
LAN: IP range start: 192.168.1.10 		Pool Count: 150
DHCP: ON

Router No.2
Model Name: Vigor2830n 
Firmware Version: 3.6.8.4_sb_232201 
Build Date/Time: 2016/01/19 18:28:17
Access: http://192.168.1.254  
Userid: admin		Password: darwin31415
Broadband Service from BT
Username: D246794@hg52.btclick.com		Password: bravo987
Phone Number: 01252 790468
Dynamic Allocation – Current Address: 31.54.142.234 [Wednesday, 25 May 2016]
DHCP: OFF


Sure Signal Device
Help Desk: 03333 040191 Ask for Sure Signal Tech Help
Serial Number: 42151520733 
MAC: B0-46-FC-80-8C-9B
Bind MAC to IP: 192.168.1.11
Controlling Mobile: 07825 290427
www.vodafone.co.uk 
Userid:	
Password: 

	

Netgear Switch
JGS516PE - 16-Port Gigabit ProSAFE Plus Switch with POE [Unmanaged]
DHCP from Router No1:	192.168.1.14	[As at Tuesday, 26 July 2016]
Access: http://192.168.1.14 
Password: password [Default in place]	
MAC: B0-7F-B9-41-B0-44
	

2860 Settings as at Tuesday, 26 July 2016
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The router is connected directly to the telephone line. 
Port 1: Netgear Switch
Port 2: Link to Router No.2
Port 4: Service to Sure Signal Device
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UPnP

Said to be necessary to enable UPnP for the Sure Signal Device to work. However it has not been enabled, which is good from a security view point, as the SSD works without this setting.
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Item 5 is the Netgear Switch
Item 6 is the Sure Signal Device
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Passwords: 
Route654
Route630
Route612
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Office VoIP Phones - All are fixed IPs with Gateway 192.168.1.254 except 200923736
 192.168.1.200		201123561 		Warehouse 
 192.168.1.201      	200920387 		Lisa
 192.168.1.202      	200923736 		Sarah O	
 192.168.1.203      	201123312 		Barnaby F		
 192.168.1.204      	201123590 		Nick S
 192.168.1.208		201123591 		Alice 
 192.168.1.209      	201123273 		Ian C 



Speed Dial:
[bookmark: OLE_LINK1][bookmark: OLE_LINK2] 10:  Warehouse	00-04-13-3B-B6-0B		201123561
[bookmark: OLE_LINK3][bookmark: OLE_LINK4] 11:  Alice		00-04-13-4D-9D-20		201123591
[bookmark: OLE_LINK5] 12:  Sarah O		00-04-13-27-6A-46  		200923736
[bookmark: OLE_LINK19][bookmark: OLE_LINK18] 13:  Carrieann O	00-04-13-36-13-4D		201123675	01252750701	8936
[bookmark: OLE_LINK6][bookmark: OLE_LINK7] 14:  Barnaby F		00-04-13-49-51-22 		201123312
[bookmark: OLE_LINK8][bookmark: OLE_LINK9] 15:  Nick S		00-04-13-41-05-D7   		201123590
[bookmark: OLE_LINK10] 16:  Ian C		00-04-13-4E-51-39   		201123273
[bookmark: OLE_LINK11] 17:  Lisa		00-04-13-4D-9D-21		200920387
[bookmark: OLE_LINK12] 18:  Walkabout		.				.		01252790468
 



	
	[image: edit] Directory

	Name:
	Number:
	Contact Type:
	Outgoing Identity:
	Edit
	Delete

	10 Warehouse
	201123561
	None
	200920387@v1.21voice.net
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	[image: delete]
	[image: dial]

	11 Alice
	201123591
	None
	200920387@v1.21voice.net
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	[image: delete]
	[image: dial]

	12 Sarah O
	200923736
	None
	200920387@v1.21voice.net
	[image: edit]
	[image: delete]
	[image: dial]

	[bookmark: _GoBack]13 Carrieann O
	201123675
	None
	200920387@v1.21voice.net
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	[image: delete]
	[image: dial]

	14 Barnaby F
	201123312
	None
	200920387@v1.21voice.net
	[image: edit]
	[image: delete]
	[image: dial]

	15 Nick S
	201123590
	None
	200920387@v1.21voice.net
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	[image: delete]
	[image: dial]

	16 Ian C
	201123273
	None
	200920387@v1.21voice.net
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	[image: delete]
	[image: dial]

	17 Lisa
	200920387
	None
	200920387@v1.21voice.net
	[image: edit]
	[image: delete]
	[image: dial]

	18 Walkabout
	01252793804
	None
	200920387@v1.21voice.net
	[image: edit]
	[image: delete]
	[image: dial]

	20 Nick Simpson Mobile
	[bookmark: OLE_LINK13]07825290427
	None
	200920387@v1.21voice.net
	[image: edit]
	[image: delete]
	[image: dial]

	[bookmark: _Hlk480042474]21 Barnaby Mobile
	07899123321
	None
	200920387@v1.21voice.net
	[image: edit]
	[image: delete]
	[image: dial]

	22 Ian C Mobile
	[bookmark: OLE_LINK16]07342880655
	None
	200920387@v1.21voice.net
	[image: edit]
	[image: delete]
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	23 Carrieann O’Connell
	07714788039
	None
	200920387@v1.21voice.net
	[image: edit]
	[image: delete]
	[image: dial]

	30 Nick Home
	[bookmark: OLE_LINK17]01252261565
	
	
	
	
	







snom Phone Setup

Within the advanced settings of each VoIP phone on the Network tab, DHCP is turned off and a fixed LAN IP address is given but maintaining the first three octaves as 192.168.1. By setting the IP Gateway as 192.168.1.254, VoIP traffic is forced to use Router No.2 thus using the alternative internet connection. A better internet connection with an up speed greater than 2Mbps would make this arrangement unnecessary. 

Typical setup shown below:
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Workgroup
Workgroup
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Callmaster Configuration [Dummy details shown]
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DrayTEL Configuration [Active but with no credit added for PAYG]
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3         192.168.1.12        94-DE-80-8D-04-19   15:17:21       EceauZoo2      
5         192.168.1.14        B0-7F-B9-41-B0-44   22:24:28                      
6         192.168.1.15        E0-3F-49-BC-E0-0A   13:37:13       EceauAsus1     
7         192.168.1.16        B4-E1-C4-E3-BE-D0   22:44:22       Windows-Phone  
8         192.168.1.18        3C-A8-2A-F6-D4-82   13:18:51       NPIF6D482      
9         192.168.1.19        94-DE-80-55-6F-6E   23:23:36       ECEAUZOO1      
10        192.168.1.22        74-D4-35-CA-62-56   12:24:37       ECEAUZOO3      
11        192.168.1.23        D8-50-E6-4A-B7-0A   23:20:01       ECEAUZOO4      
12        192.168.1.39        D8-CB-8A-EC-98-AD   14:43:58       ECEAUSERVER    

BT Business Hub; How to convert to modem mode
http://btbusiness.custhelp.com/app/answers/detail/a_id/35226/~/how-do-i-enable-bridge-mode-on-my-bt-business-hub-5%3F

How do I enable bridge mode on my BT Business Hub 5?
To enable bridging mode on the BT Business Hub 5:
1. On a PC or laptop connected to your hub, enter http://btbusinesshub.home or 192.168.1.254
2. Click on Advanced Settings
3. Enter your Admin password if prompted (can be found on the base of your Hub) and click Ok
4. Click Continue to Advanced Settings
5. Choose the Broadband tab, then click on the Routing tab
6. Scroll down to the bottom of the page to Bridging
7. Tick Yes next to Enabled
8. If you're sure click Yes on the next screen
Your BT Business Hub should now be in bridge mode. You will need to change the settings on your other Router to use connection type PPPoE. Depending on the Hub you are bridging to, you may need to enter your broadband connection details.
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Vigor2860Vac

VDSL2 Securiy Firewoll

[

Model Name Vigor2860Vac System Up Time |361:20:6 System Status
Router Name Nol Current Time 2016 Aug 5 Fri 11:25:14 Dynamic DNS
Firmware Version |3.8.2.3_BT Build Date/Time | Apr 22 2016 10:28:07 TR069
DSL Version 576D17_A/B/C HW: A LAN MAC Address | 00-1D-AA-E6-CB-E6 User Management

IM/P2P Block

Schodule

Line | Mode 1P Address MAC Address SysLog / Mail Alert
WAN1_| VDSL2 / PPPOE 81.136.214.64 | 00-1D-AA-E6-CB-EQ LDAP
WAN2 | Ethernet / DHCP. onnected 00-1D-AA-E6-CB-EA RADIUS
WANS | USB/ - Disconnected 00-1D-AA-E6-CBEB
WANZ [USB/ onnected 00-1D-AA-E6-CB-EC Data Flow Monitor

Connected : Down Stream : 17538Kbps / Up Stream : 1177Kbps
WAN | Connected : 1, @WANI __WAN2 __WAN3 __WAN#
O LAN Connected : 9, @LANL _@LAN2 LAN3  @LAN4 LANS LANG
J WLAN _| Connected : 0
3 WLANSG| Connected : 0
0, _UsB1
use 0, _uss2

3 VPN Connected :

Remote Dial-in User

nUser / LAN to LAN

3 MyVigor | Activate : 0

Profile In/Out
Phone1 Callmaster No 0/0
Phone2 Callmaster No 0/0
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WAN >> General Setup

WAN 1
Enable: Yes v
Display Name: BT1
Physical Mode: vDsL2
DSL Mode: Auto v
Physical Type: Auto negotiation v
DSL Modem Code: Default Vi
Line Speed(Kbps):
DownLink 0
UpLink 0
VLAN Tag insertion (ADSL):  [Disable
Tag value: 0 (0~4095)
priority: 0 (0~7)
VLAN Tag insertion (VDSL2): [Enable V|
Tag value: 101 ] (0~4095)
priority: 0 (0~7)
Active Mode: [Always On V| Load Balance: M
Note:

1. The line speed setting of WAN interface is available only when According to Line Speed is selected
as the Load Balance Mode.

2. In DSL auto mode, the router will reboot automatically while switching between VDSL2 and ADSL
lines.
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WAN >> Internet Access

Internet Access

Index Display Name Physical Mode

WANL BTL ADSL / VDSL2
WAN2 Ethernet
WAN3 usB.
WAN4 uss

Access Mode

PPPOE | PPPoA V] [ Details Page | [ 1Pve
Static or Dynamic IP V] [ Details Page | [ 1Pve
None V] | Details Page | [ 1Pve
None V] | Details Page | [ 1Pve

Note: 1. Device on USB port 1 applies WAN3 configuration.
Device on USB port 2 applies WAN4 configuration.
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WAN >> Internet Access

WAN 1
PPPOE | PPPoA MPoA / Static or Dynamic IP 1Pv6

Disable ISP Access Setup

) Enable

Service Name

Modem Settings (for ADSL only)

Multi-PVC channel Channel 1 V]| username D458423@hg70 bciick
ve1 0 Password

ver 38 [JFallback account

Encapsulating Type VCMUX v Fallback Username

protocol PPPoA v Fallback Password

Modulation Multimode Vi

[separate Account for ADSL
PPPOE Pass-through

[ For wired LAN®
[ For wireless LAN

PPP Authentication [PAP or CHAP V|
1P Address From ISP [ WAN IP Alias

WAN Connection Detection Fixed IP Yes ©® No (Dynamic IP)

Mode ARP Detect V| Fixed IP Address

MTU 1520 ] (Max:1520) © Default MAC Address
Path MTU Discovery | Detect © Specify a MAC Address
MAC Address: 00 | -[1D] {AA {E6 | {CB] |E9
Index(1-15) in_Schedule Setup:
=> | 3 3
Notes

1: (Optional) Required for some ISPs. Leave blank if in doubt because the connection request
might be denied if "Service Name" is incorrect.

2: If this box is checked while using the PPPOA protocol, the router will behave like a modem which
only serves the PPPOE client on the LAN,
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Applications >> UPnP

UPnP

[J Enable UPNP Service Default WAN Vv
Enable Connection Control Service

Enable Connection Status Service

Note:To allow NAT pass-through to a UPnP enabled client the connection control service must also be
enabled.
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System Maintenance >> SysLog / Mail Alert Setup

SysLog / Mail Alert Setup

SysLog Access Setup

Enable

Syslog Save to:
Msyslog Server

[luse pisk
Router Name Not
Server IP Address 192168112
Destination Port 514
Mail Syslog MEnable

Enable syslog message:
M Firewall Log
] VPN Log
] User Access Log
M call Log
] WAN Log

¥ Router/DSL information
AlertLog Setup

MEnable
AlertLog Port 514

Mail Alert Setup
MlEnable
SMTP Server
SMTP Port
Mail To
Return-path
Ml use ssL
¥ Authentication
Username
password
Enable E-Mail Alert:
¥ Dos Attack
I apPe
I ven Log
[ APPE signature

Send a test e-mail

1526 sovdns com
465
david@cyberpictures n

eceau@cyberpictures 1

eceau@cyberpictures 1

Note: 1. Mail Syslog cannot be activated unless USB Disk is

2. Mail Syslog feature sends a Syslog file when its size reaches 1M Bytes
3. We only support secured SMTP connection on port 465.

ked for "Syslog Save to".
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rewall >> General Setup

General Setup

General Setup Default Rule

Call Filter Enable Start Filter Set [Set#1_v|

Disable
Enable Start Filter Set [Set#2 V|

Data Filter

Disable

Accept large incor
streaming)

Enable Strict Security Firewall
Block routing packet from WAN
Ceva ™ 1pve

g fragmented UDP or ICMP packets (used in some games and

Note: The packets will be filtered by the following firewall functions sequentially:
1. Data Filter Sets and Rules
2. Block routing packets from WAN
3. Default Rule
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Diagnostics >> View DHCP Assigned IP Addresses

DHCP IP Assignment Table

DHCPv6 IP Assignment Table

| Refresh |

168.
168.
168.
168.
168.
168.
168.
168.
168.
168.
168.
168.
168.

1.
J11
12
.13
.14
.15
.16
.18
.19
22
.23
.24
.39

T

192.168.1.1/255.255.255.0,
IP Address
192.
192.
192.
192.
192.
192.
192.
192.
192.
192.
192.
192.
192.

10

MAC Address
38-F2-3E-A8-03-68
E0-3F-49-BC-E0-0A
94-DE-80-8D-04-19
Interface: 10
BO-7F-B9-41-B0-44
18-F6-43-DB-13-69
B0-46-FC-80-8C-9B
3C-A8-2A-F6-D4-82
94-DE-80-55-6F-6E
74-D4-35-CA-62-56
D8-50-E6-4A-B7-0A
78-E3-B5-AF-DI-22
D8-CB-8A-EC-98-AD

DHCP server: On

Comment

HOST ID
Windows-Phone
Eceaussusl
Eceauzoo2
VEN-1

TravissiPhone2

NPIF6D482
ECEAUZOOL
ECEAUZ003
ECEAUZ004
Eceau2-HP
ECEAUSERVER
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Online Status

Physical Connection System Up days 0:38:16
1Pv4 1Pve
LAN Status Primary DNS: 62.6.40.162 Secondary DNS: 194.74.65.69
1P Address TX Packets RX Packets
192.168.1.1 14629552 22682268
[WAN 1 Status >> Drop PPPoE
Enable Line Name Mode Up Time
Yes vDsL2 BT1 PPPOE 120:37:13
13 GWIP TXPackets  TXRate(Bps) ~ RXPackets  RX Rate(Bps)
81.136.214.64 _ 81.148.160.1 10860083 24837 11180142 23452
[WAN 2 Status >> Renew
Enable Line Name Mode Up Time
Yes Ethernet DHCP Client  00:00:00
13 GWIP TXPackets  TXRate(Bps) ~ RXPackets  RX Rate(Bps)
- [ 0 [ o
[WAN'3 Status
Enable Line Name Mode Up Time signal
Yes uss 00:00:00 -
13 GWIP TXPackets  TXRate(Bps) ~ RXPackets  RX Rate(Bps)
- [ 0 [ o
[WAN 4 Status
Enable Line Name Mode signal
Yes uss -
P GWIP TXPackets  TXRate(Bps) ~ RXPackets  RX Rate(Bps)
- [ 0 [ o

[VDSL2 Information
Pre State
17A

SHOWTIME

(VDSL2 Firmware Version: 576D17_A/B/C with Vectoring support )
SNR Upstream
6 (dB)

UP Speed
1185 (Kbps)

Down Speed
17707 (Kbps)

SNR Downstream
5 (dB)
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Diagnostics >> View ARP Cache Table

Show: [ALLLANs V] and [ALLVLANSs V|
Ethernet ARP Cache Table | Clear | Refresh |
Ip Address MAC Address Netbios Name Interface VIAN Porc
192.169.1.200 00-04-13-35-56-08 LaNL P1
192.169.1.201 00-04-13-2D-9D-21 LaNL P1
192.169.1.202 00-04-13-27-6A-46 LaNL P1
192.169.1.203 00-04-13-29-51-22 LaNL B1
192.169.1.20¢ 00-04-13-41-05-D7 LaNL P1
192.169.1.206 00-04-13-42-51-33 LaNL P1
192.169.1.25¢ 00-1D-3A-E5-62-08 LaNL P2
s192.168.1.11 50-26-FC-20-3C-95 LaNL 25
192.168.1.12 54-DE-80-8D-04-18 ECEADZO02 LaNL P1
192.168.1.1¢ 50-7F-B9-41-50-4¢ LaNL P1
192.168.1.18 3C-28-23-F6-D-52 LaNL P1
192.168.1.18 54-DE-30-55-6F-62 ECEADZOOL LaNL P1
192.169.1.22 74-D4-35-Ca-62-56 ECEADZO003 LaNL P1
192.169.1.23 D8-50-E6-4A-B7-02 LaNL B1
192.169.1.39 DS-CB-8A-EC-93-AD  ECEAUSERVER LaNL B1
< >
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Wireless LAN(2.4GHz) >> General Setup

General Setting ( IEEE 802.11)

Enable Wireless LAN

Mode : Mixed(11b+11g+11n) v/
Channel: Channel 4, 2427MHz v/
Enable Hide SSID ssID Isolate Member Isolate VPN
1 o Eceau o [m)
2 ™ o Eceau-Guest
3 O
4 0O
Note:

Enabling the Isolate Member configuration will forbid the wireless clients associated to
the same SSID from connecting to each other.

The isolate VPN configuration will isolate the wireless traffic from VPN connections and
thus, wireless clients will not be able to access the VPN network under this setting.
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Wireless LAN(5GHz) >> General Setup

General Setting ( IEEE 802.11)

Enable Wireless LAN
Mode :
Channel:

Mixed (11a=11n+11ac) V]

Channel 36, 5180MHz V|

Enable Hide SSID ssID Isolate Member Isolate VPN
1 [m] Eceaus o [m)
2 O
3 O
4 0O
Note:

Enabling the Isolate Member configuration will forbid the wireless clients associated to
the same SSID from connecting to each other.

The isolate VPN configuration will isolate the wireless traffic from VPN connections and
thus, wireless clients will not be able to access the VPN network under this se
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LAN >> General Setup

General Setup

Index Status  DHCP  IP Address,
LAN 1 v v 102.168.1.1 Details Page 1Pv6
LAN 2 ¥ 102.168.2.1 Details Page 1Pv6
LAN 3 2 102.168.3.1 Details Page 1Pv6
LAN 4 ¥ 102.168.4.1 Details Page 1Pv6
LAN 5 2 102.168.5.1 Details Page 1Pv6
LAN 6 ¥ 102.168.6.1 Details Page 1Pv6
DMZ Port O o 192.168.7.1 Details Page 1Pv6
1P Routed Subnet =] 2 192.168.0.1 Details Page
Advanced [¥ou can configure DHCP server options here.
[JForce router to use "DNS server IP address" settings specified in LANT v
Inter-LAN Routing
Subnet LAN1 LAN2 LANZ LAN4 LANS LANG  DMZPort
LAN 1 v
LAN 2 v
LaN 3 v
Lan 4 ~
LaN S <
LaN & <
DMZ Port =] v

Note: LAN 2/3/4/5/6 are available when VLAN
DMZ subnet is default bound to P1, and

ings of P1 at LAN> >VLAN p:

age.
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LAN >> General Setup

LAN 1 Ethernet TCP / IP and DHCP Setup

LAN 11PV6 Setup

Network Configuration
For NAT Usage

1P Address 192.168.1.1
Subnet Mask [255.255.255.0
RIP Protocol Control Disable v/

DHCP Server Configuration

Enable Server
[JEnable Relay Agent
Start IP Address

1P Pool Counts
Gateway IP Address
Lease Time

[ Clear DHCP lease for
periodically

) Disable Server

192.168.1.10

150

192.168.1.1

86400

()

inactive clients

DNS Server IP Address
Primary 1P Address
Secondary IP Address
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System Maintenance >> Management

IPv4 Management Setup

1Pv6 Management Setup

Router Name Not

M Default:Disable Auto-Logout
[ Enable Validation Code in Internet/LAN
Access

Note: DrayOS CAPTCHA is not supported in
Safari or IE versions 8 and below.

Internet Access Control

M Allow management from the Internet
Domain name allowed

[ FTP server
¥ HTTP Server
¥ HTTPS Server
[ Telnet server
[ TRO69 Server
[ ssH server
[ pisable PING from the Internet

LAN Access Control
M Allow management from LAN
M FTP server
M HTTP server
M HTTPS Server
¥ Telnet server

[Vl ssH server
Apply To Subnet

MLaN2 M LaN3 M LAN4 M LANS
¥pMz M1p Routed Subnet

LANG

Management Port Setup

® User Define Ports C

Default Ports

Telnet Port 23 (Default: 23)
HTTP Port 8080 ] (Default: 80)
HTTPS Port 443 (Default: 443)
FTP Port 21 (Default: 21)
TRO69 Port 8069 | (Default: 8069)
SSH port 22 (Default: 22)
TLSISSL Encryption Setup

[JEnable ssL 3.0

CVM Access Control

ClevM port 8000 | (Default: 8000)
[Clcvm ssi port 8443 | (Default: 8443)

MDevice Management

[Respond to external device
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Access List from the Internet

List » Subnet Mask

1 Vi
2 Vi
3 Vi

Note: Subnet LANT is always allowed to access all the router services regardless of "LAN Access
Control” settings.
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LAN >> Bind IP to MAC

Bind IP to MAC

Enable O Disable O Strict Bind

ARP Table | SelectAll | Sort | Refresh | IP Bind List ( Limit: 300 entries ) | Select All | Sort |
T Acaress Vac Address Tnaex TP Aadzess Comment
152.168.1.200  00-04-13-38-86-08 A| |1 162.168.1.11  Sure Signal
152.168.1.201  00-04-13-4D-9D-21
152.168.1.202  00-04-13-27-6A-46
152.168.1.203  00-08-13-29-51-22
152.168.1.204  00-04-13-41-05-D7
152.168.1.206  00-04-13-4E-51-33
152.168.1.254  00-1D-AA-BB-62-08
152.168.1.11  B0-6-FC-20-8C-98 V|
152.168.1.12  94-DE-30-8D-03-19
Add or Update
1p Address
Mac Address
Comment
¥ Show Comment
Add | [ Updete | [ Delete

Note:  IP-MAC binding presets DHCP Allocations.

If you select Strict Bind, unspecified LAN clients cannot access the Internet.
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Network

Behavior ~ Audio ~ SIP/RTP  QoS/Security

Update

Network:
DHCP:

1P address:
Netmask

Host Nam
1P Gateway:

i @
192.168.1.200
255.255.255.0

192.168.1.254

EEINC)
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VolP >> General Settings

¥ Enable voIp

Note
During the VoIP disable:(1)For the models that has line port interface, the FXS ports will
connect to line port. (2)For the models that does not have line port, the FXS ports will be
turned off that is no power supplied in FXS ports.

Secure Phone
[ Enable Secure Phone (ZRTP+SRTP)
™ Enable SAS Voice Prompt

NAT Traversal Setting

STUN Server

External Ip
SIP PING Interval 150 sec

RTP
0 symmetric RTP
Dynamic RTP Port Start 10050
Dynamic RTP Port End 15000
RTP TOS IP precedence 5 | 10100000

1P Call
M Enable 1P Call
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VolP >> DialPlan Setup

(2]

Phone Book Digit Map Call Barring Regional PSTN Setup
# Enable MatchPrefix  Mode  OPNumber  |Un VX goute MJ¥e piove
1 2500 Replace V] 8500 i VolPT V| Down
2 B Replace V] 6 5 7 VolPZ v UP  Down
3 5 None v i g VoPT V| UP  Down
4 0 Replace ] [0 11 |[11_|[PSTN v] UP Down
s i Replace V] [1 g 5 VolPT V] UP  Down
5 2 Replace V] [2 g g VolPT V] UP Down
7 @[ Replace V] [141 15 |14 |[VoP2 ¥] UP Down
s @ [o2 None v g B VolPz V| UP  Down
9 & [e None v g B PSTN V| UP Down
0 & [0 None v g B PSTN V| UP Down
1 1471 None v il PSTN V| UP  Down
12 710 Replace v/ [201123561 g 5 VoPT V] UP  Down
13 1 Replace v/ [200920387 g 5 VolPT V] UP  Down
14 712 Replace v/ [200923736 g 5 VolPT V] UP Down
15 713 Replace V] [201123312 g 5 VolPT V] UP  Down
16 714 Replace V] [201123273 g 5 VolPT V] UP Down
17 715 Replace V] [201123590 g 5 VolPT V] UP  Down
18 @ [716 Replace v/ [201123591 g 5 VolPT V] UP Down
19 & [ Replace V] [200820253 g B VolPT V| UP  Down
20 O Replace V! 0 0 PSTN V| UP

Note: 1. The length for Min Len and Max Len fields should be between 0~25.

2. Wildcard 7' is supported.
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