Router & VoIP Configuration at Robanes
Thursday, 14 February 2013
Access to the router is through IP address 192.168.40.1 where the logon credentials are david/elstead2008.

Following configuration the system and online status pages were examined and report the following.  The firmware version is slightly dated but what would be gained in upgrading is unknown.
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192.168.40.1 2200368 1418347
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Out of the box, the router immediately synced up with the O2 service and reported that the modulation mode was ADSL2+ (G.992.5) and was reporting an up and down speed as estimated at the time of the order.
Definitive information on the configuration settings for the router was difficult to determine so initially auto configuration was allowed to kick in with the only manual input being the fixed IP address. Whereas additional configuration settings can be entered, these were rejected by the router.
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The configuration shown above is different to the example provided but as an internet service was obtained there seemed little point in changing anything. The default LAN settings were replaced with 192.168.40.xx and a new password provided for access to the router.
Short codes were set up to match the existing phone system as shown below.
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The Wireless functionality was enabled and populated as shown below
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The PSK was set as route654

A check was made to ensure that the channel selected did not conflict with other nearby services,
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To allow for remote management a emote Dial-in user account was created.
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Finally a back up of the configuration settings was made.

Connected to the LAN are three PCs, two SIP phones, a networked printer and a storage device. Apart from the router there are no fixed IP addresses. All devices are connected to the switch except the storage device.

Driver software was downloaded for the printer to use with Windows7 PCs and the installation disk was used for the Xp machine.  Previously the printer was setup via a USB port.

The Work group for all machines was set to Pictures and the names of the PC’s changed.
The SIP phones function keys were configured for extension to extension calling as shown below. 
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Barry’s Phone





Neil’s Phone
Post installation activities have been to move stored emails and the contacts list over to Outlook2010 and also the bookmarks of Internet Explorer. 

Outstanding activates requiring attention:

1. Shut down the BT Broadband service and ensure future payments are not made.

2. Organise the transfer of 01622 664200 over to VoIP [Safe to do so]
There are 4 analogue lines associated with this number with 3 feeds into the switch and the other to a master socket. Possibility that DDI numbers exist which could be preserved 
3. Ensure there is a DD in place for the O2 Broadband service

4. Consider Total Care for the line 01622 750754

5. Removal of switch and analogue telephone instruments connected to the switch

