Computer Installation – Katherine Wills
Last Update: Thursday, 22 June 2017

Home Address:
21 Poplar Walk
Farnham
Surrey 
GU9

Telephone:	01252 724054
Mobile: 	07979 713175

Broadband ISP:  SKY	Speed:  40/10
Last know WAN address:  151.224.34.45
LAN IP: 192.168.0	Start: 2		End: 254		Lease Time: ?
Remote Management: ON		Only Allowed:  everyone		Port No.: 8080
[bookmark: OLE_LINK1][bookmark: OLE_LINK2][bookmark: _GoBack]Router: 192.168.0.1		Remote Access http://151.224.34.45:8080/
Username: admin		Password: PoplarWalk	

Workgroup: HALE

Wireless SSID: SKYAA373	Channel: 11	Password: CVBQRXEA		Security: WPA2 -PSK 

Location of WAN addresses used in these notes
Dynamic Home		151.224.34.45
Fixed AVEUK		81.136.145.37
Fixed David Bradley


Attached Devices

		#
	IP Address
	Device Name
	MAC Address

	1
	192.168.0.2
	Katherine-PC
	90:2b:34:b4:b9:b1

	2
	192.168.0.20
	snom162
	00:04:13:29:8a:d0

	3
	192.168.0.5
	NPI6A288F
	38:ea:a7:6a:28:8f

	4
	192.168.0.8
	Wii
	00:23:31:e4:c7:88

	5
	192.168.0.6
	Ellies-iPod
	c0:63:94:95:15:1a

	6
	192.168.0.4
	jamys-ipod
	88:c6:63:5f:55:25




	Address Reservation

		#
	IP Address
	Device Name
	MAC Address

	1
	192.168.0.11
	snom162
	00:04:13:29:8a:d0

	2
	192.168.0.5
	NPI6A288F
	38:ea:a7:6a:28:8f




	NOTE: Address reservation created to ensure that the snom phone and printer always have the same IP address.

Firewall Rules - Outbound Services

		#
	Enable
	Service Name
	Action
	LAN Users
	WAN Servers
	Log

	Default
	Yes
	Any
	ALLOW always
	Any
	Any
	Never



Firewall Rules – Inbound Services

	
		#
	Enable
	Service Name
	Action
	LAN Server IP address
	WAN Users
	Log

	1
	
	Printing
	ALLOW always
	192.168.0.5 (9100:9100)
	0.0.0.0 (1:65535)
	Always

	Default
	Yes
	Any
	BLOCK always
	Any
	Any
	Never








NOTE: No inbound service to the snom phone configured. Printing is enabled to allow RDC sessions to AVE to print on the local printer. WAN users set to ANY to allow DCB or SRB access to the printer.
Services Table
		#
	Service Type
	Ports

	1
	snom
	80..80

	2
	Printing
	9100...9100





Snom identity 200921162 - Rings on 01252 733200	DDI: 01252 739162 
WAN Access: 
Logon Userid to GUI:  queen		Password:  bee4	Administrator: 
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