On the network as 192.168.0.106
QR Code: t4UJtC

Step-by-Step Setup:
1. Power the Access Point: 
Connect the UniFi AP to a compatible Power over Ethernet (PoE) switch or a PoE adapter using an Ethernet cable. 
2. Download the App: 
Install the UniFi Network app on your mobile device from the Apple App Store or Google Play Store. 
3. Connect to the Network: 
Ensure your smartphone is connected to the same local network as the powered-on access point. 
4. Launch the App & Adopt Device:
. Open the UniFi Network app. 
. If setting up standalone (without a UniFi console), you can use Bluetooth to find the AP and initiate setup. 
. Alternatively, if the AP is discoverable on your network, select the "Add Device" option or the device icon (⋮). 
. Scan the QR code on the back of the access point or enter the serial number manually to identify it. 
5. Configure Settings: 
Follow the on-screen instructions to name the access point, set up your Wi-Fi network name (SSID), and establish a password for your wireless network. 
6. Complete Setup: 
The AP will provision the settings and connect to your network, providing immediate access to the fast Wi-Fi 6 speeds. 
Key Considerations:
· Standalone vs. Controller: 
You can set up the AP in "Standalone Mode" for instant network access without needing to create a full UniFi account, or you can adopt it into a UniFi Network application (self-hosted or on a UniFi Console) for more advanced management and features. 
· Bluetooth Setup: 
The UniFi Network app uses Bluetooth for initial device discovery and adoption, especially useful for standalone setups, according to this YouTube video. 
